**Pseudo Code**

Initialize PortF

Load PortF Data Address

Load PortF Data

Isolate Input Pins

Isolate SW1

Move SW1 bit to common position

Isolate SW2

Move SW2 bit to common position

Check if either is on

Move Result to LED

Insert Result

Move to other LED

Insert Result

Reload Data Register Address

Toggle LED's accordingly

Loop Back



